{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["废气","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"废气","index":0,"n_rows":106,"n_cols":9,"rows_kept":106,"merged":[[1,0,1,8],[3,0,39,0],[3,1,39,1],[3,2,5,2],[3,3,11,3],[3,4,5,4],[6,4,9,4],[7,2,9,2],[10,2,11,2],[10,4,11,4],[12,2,18,2],[12,3,18,3],[12,4,18,4],[19,2,25,2],[19,3,25,3],[19,4,25,4],[26,2,32,2],[26,3,32,3],[26,4,32,4],[33,2,39,2],[33,3,39,3],[33,4,39,4],[40,0,47,0],[40,1,47,1],[40,2,42,2],[40,3,47,3],[40,4,43,4],[44,2,46,2],[44,4,47,4],[48,0,51,0],[48,1,51,1],[48,2,50,2],[48,3,51,3],[48,4,51,4],[52,0,55,0],[52,1,55,1],[52,2,54,2],[52,3,55,3],[52,4,55,4],[56,0,62,0],[56,1,62,1],[56,2,58,2],[56,3,62,3],[56,4,58,4],[59,2,61,2],[59,4,62,4],[63,0,66,0],[63,1,66,1],[63,2,65,2],[63,3,66,3],[63,4,66,4],[67,0,73,0],[67,1,73,1],[67,2,69,2],[67,3,73,3],[67,4,73,4],[71,2,73,2],[74,0,97,0],[74,1,97,1],[74,2,80,2],[74,3,81,3],[74,4,81,4],[82,2,83,2],[82,3,85,3],[82,4,95,4],[84,2,85,2],[86,2,90,2],[86,3,97,3],[91,2,95,2],[96,4,97,4],[98,0,101,0],[98,1,101,1],[98,2,100,2],[98,3,101,3],[98,4,101,4],[102,2,102,8],[103,2,103,8],[104,1,104,8],[105,1,105,8]],"flags":["formulas_cached_only"]}
["附件2"]
["广州市2018年国控企业污染源（废气重点）监督性监测结果（12月）"]
["行政区","企业名称","监测点名称","执行标准名称","监测日期","监测项目名称（单位）","污染物浓度","标准限值","是否达标"]
["黄埔区","中国石油化工股份有限公司广州分公司","3#220t/h锅炉处理后","《火电厂大气污染物排放标准》（GB13223-2011）表2大气污染物特别排放限值","2018-11-20","氮氧化物(mg/m3)",10,100,"是"]
[{"$nulls":5},"二氧化硫(mg/m3)",8,50,"是"]
[{"$nulls":5},"汞及其化合物(mg/m3)","ND(0.0025)",0.03,"是"]
[null,null,"3#、4#220t/h锅炉烟囱排放口",null,"2018-11-16","林格曼黑度（级）",0.5,1,"是"]
[null,null,"4#220t/h锅炉处理后",null,null,"氮氧化物(mg/m3)",17,100,"是"]
[{"$nulls":5},"二氧化硫(mg/m3)",11,50,"是"]
[{"$nulls":5},"汞及其化合物(mg/m3)","ND(0.0025)",0.03,"是"]
[null,null,"1#、2#CFB炉排放口",null,"2018-11-22","氮氧化物(mg/m3)",13,100,"是"]
[{"$nulls":5},"二氧化硫(mg/m3)","ND（3）",50,"是"]
[null,null,"炼油区下风向边界点1#","《石油炼制工业污染物排放标准》（GB31570-2015）表5企业边界大气污染物排放限值","2018-11-21","总悬浮颗粒物(mg/m3)",0.296,{"v":1,"d":"1.0"},"是"]
[{"$nulls":5},"苯并[a]芘(mg/m3)","ND(5×10-8)",8e-06,"是"]
[{"$nulls":5},"非甲烷总烃(mg/m3)",0.34,{"v":4,"d":"4.0"},"是"]
[{"$nulls":5},"氯化氢(mg/m3)",0.18,0.2,"是"]
[{"$nulls":5},"甲苯(mg/m3)",0.018,0.8,"是"]
[{"$nulls":5},"苯(mg/m3)","ND(0.002)",0.4,"是"]
[{"$nulls":5},"二甲苯(mg/m3)",0.022,0.8,"是"]
[null,null,"炼油区下风向边界点2#","《石油炼制工业污染物排放标准》（GB31570-2015）表5企业边界大气污染物排放限值","2018-11-21","总悬浮颗粒物(mg/m3)",0.293,{"v":1,"d":"1.0"},"是"]
[{"$nulls":5},"苯并[a]芘(mg/m3)","ND(5×10-8)",8e-06,"是"]
[{"$nulls":5},"非甲烷总烃(mg/m3)",0.23,{"v":4,"d":"4.0"},"是"]
[{"$nulls":5},"氯化氢(mg/m3)",0.14,0.2,"是"]
[{"$nulls":5},"甲苯(mg/m3)","ND(0.001)",0.8,"是"]
[{"$nulls":5},"苯(mg/m3)","ND(0.002)",0.4,"是"]
[{"$nulls":5},"二甲苯(mg/m3)","ND(0.001)",0.8,"是"]
[null,null,"化工区下风向边界点1#","《石油化学工业污染物排放标准》（GB31571-2015）表7企业边界大气污染物排放限值","2018-11-21","总悬浮颗粒物(mg/m3)",0.112,{"v":1,"d":"1.0"},"是"]
[{"$nulls":5},"苯并[a]芘(mg/m3)","ND(5×10-8)",8e-06,"是"]
[{"$nulls":5},"非甲烷总烃(mg/m3)",{"v":0.4,"d":"0.40"},{"v":4,"d":"4.0"},"是"]
[{"$nulls":5},"氯化氢(mg/m3)",0.17,0.2,"是"]
[{"$nulls":5},"甲苯(mg/m3)",{"v":0.02,"d":"0.020"},0.8,"是"]
[{"$nulls":5},"苯(mg/m3)","ND(0.002)",0.4,"是"]
[{"$nulls":5},"二甲苯(mg/m3)",0.022,0.8,"是"]
[null,null,"化工区下风向边界点2#","《石油化学工业污染物排放标准》（GB31571-2015）表7企业边界大气污染物排放限值","2018-11-21","总悬浮颗粒物(mg/m3)",0.541,{"v":1,"d":"1.0"},"是"]
[{"$nulls":5},"苯并[a]芘(mg/m3)","ND(5×10-8)",8e-06,"是"]
[{"$nulls":5},"非甲烷总烃(mg/m3)",0.32,{"v":4,"d":"4.0"},"是"]
[{"$nulls":5},"氯化氢(mg/m3)",0.13,0.2,"是"]
[{"$nulls":5},"甲苯(mg/m3)","ND(0.001)",0.8,"是"]
[{"$nulls":5},"苯(mg/m3)","ND(0.002)",0.4,"是"]
[{"$nulls":5},"二甲苯(mg/m3)","ND(0.001)",0.8,"是"]
["南沙区","互太（番禺）纺织印染有限公司","1#、2#、3#锅炉处理后","《火电厂大气污染物排放标准》（GB13223-2011）表2大气污染物特别排放限值（燃煤锅炉）","1#、2#锅炉已拆除，3#锅炉停开","二氧化硫(mg/m3)","/",50,"/"]
[{"$nulls":5},"氮氧化物(mg/m3)","/",100,"/"]
[{"$nulls":5},"汞(mg/m3)","/",0.03,"/"]
[null,null,"1#、2#、3#锅炉烟囱排放口",null,null,"林格曼黑度(级)","/",1,"/"]
[null,null,"4#、5#、6#锅炉处理后",null,"2018-11-20","二氧化硫(mg/m3)",11,50,"是"]
[{"$nulls":5},"氮氧化物(mg/m3)",35,100,"是"]
[{"$nulls":5},"汞(mg/m3)","ND（0.0025）",0.03,"是"]
[null,null,"4#、5#、6#锅炉烟囱排放口",null,null,"林格曼黑度(级)",0.5,1,"是"]
["南沙区","广州华润热电有限公司","1#30万千瓦发电机组处理后","《火电厂大气污染物排放标准》（GB13223-2011）表2大气污染物特别排放限值（燃煤锅炉）","2018-11-23","二氧化硫(mg/m3)",9,50,"是"]
[{"$nulls":5},"氮氧化物(mg/m3）",27,100,"是"]
[{"$nulls":5},"汞(mg/m3)","ND(0.0025)",0.03,"是"]
[null,null,"1#30万千瓦发电机组处理后烟囱排放口",null,null,"林格曼黑度（级）",0.5,1,"是"]
["南沙区","广州华润热电有限公司","2#30万千瓦发电机组处理后","《火电厂大气污染物排放标准》（GB13223-2011）表2大气污染物特别排放限值（燃煤锅炉）","停炉维修","二氧化硫(mg/m3)","/",50,"/"]
[{"$nulls":5},"氮氧化物(mg/m3）","/",100,"/"]
[{"$nulls":5},"汞(mg/m3)","/",0.03,"/"]
[null,null,"2#30万千瓦发电机组处理后烟囱排放口",null,null,"林格曼黑度（级）","/",1,"/"]
["黄埔区","广州恒运热电（D）厂有限责任公司","9#（30万千瓦）锅炉\n处理后","《火电厂大气污染物排放标准》（GB13223-2011）表2大气污染物特别排放限值（燃煤锅炉）","2018-11-19","二氧化硫（mg/m3）",16,50,"是"]
[{"$nulls":5},"氮氧化物（mg/m3）",40,100,"是"]
[{"$nulls":5},"汞及其化合物（mg/m3）","ND(0.0025)",0.03,"是"]
[null,null,"8#（30万千瓦）锅炉\n处理后",null,"2018-11-21","二氧化硫（mg/m3）",16,50,"是"]
[{"$nulls":5},"氮氧化物（mg/m3）",43,100,"是"]
[{"$nulls":5},"汞及其化合物（mg/m3）","ND(0.0025)",0.03,"是"]
[null,null,"8#、9#(30万千瓦)锅炉烟囱排放口",null,null,"林格曼黑度（级）",0.5,1,"是"]
["黄埔区","广州恒运企业集团股份有限公司","6#、7#锅炉处理后","《火电厂大气污染物排放标准》（GB13223-2011）表2大气污染物特别排放限值（燃煤锅炉）","2018-11-19","二氧化硫（mg/m3）",21,50,"是"]
[{"$nulls":5},"氮氧化物（mg/m3）",34,100,"是"]
[{"$nulls":5},"汞及其化合物（mg/m3）","ND(0.0025)",0.03,"是"]
[null,null,"6#、7#锅炉烟囱排放口",null,null,"林格曼黑度（级）",0.5,1,"是"]
["增城区","广州市旺隆热电有限公司","1#420t/h锅炉处理后","《火电厂大气污染物排放标准》（GB13223-2011）表2大气污染物特别排放限值（燃煤锅炉）","停产","二氧化硫(mg/m3)","/",50,"/"]
[{"$nulls":5},"氮氧化物(mg/m3)","/",100,"/"]
[{"$nulls":5},"汞及其化合物(mg/m3)","/",0.03,"/"]
[null,null,"1#、2#420t/h锅炉处理后烟囱排放口",null,null,"林格曼黑度（级）","/",1,"/"]
[null,null,"2#420t/h锅炉处理后",null,null,"二氧化硫(mg/m3)","/",50,"/"]
[{"$nulls":5},"氮氧化物(mg/m3)","/",100,"/"]
[{"$nulls":5},"汞及其化合物(mg/m3)","/",0.03,"/"]
["花都区","广州市越堡水泥有限公司","回转窑尾","《水泥工业大气污染物排放标准》(GB 4519-2013)表1 现有与新建企业大气污染物排放限值+广东省《水泥工业大气污染物排放标准》(DB44 818-2010)表2规定的大气污染物最高允许排放限值+《水泥窑协同处置固体废物污染控制标准》表1协同处置固体废物水泥窑大气污染物最高允许排放浓度\n","2018-11-22","*颗粒物（烟尘）(mg/m3)","<20",30,"/"]
[{"$nulls":5},"氮氧化物（mg/m3）",232,400,"是"]
[{"$nulls":5},"二氧化硫（mg/m3）",12,100,"是"]
[{"$nulls":5},"汞（mg/m3）","ND(0.0025)",0.05,"是"]
[{"$nulls":5},"氟化氢（mg/m3）",0.52,1,"是"]
[{"$nulls":5},"氟化物（mg/m3）","ND(0.06)",3,"是"]
[{"$nulls":5},"氨（mg/m3）",3.44,10,"是"]
[null,null,"回转窑尾烟囱排放口",null,null,"林格曼黑度（级）",0.5,"/","/"]
[null,null,"下风向边界点1#","《水泥工业大气污染物排放标准》(GB 4519-2013)表3 大气污染物无组织排放限值+广东省《水泥工业大气污染物排放标准》(DB44 818-2010)表3作业场所颗粒物无组织排放限值","2018-11-22","总悬浮颗粒物（mg/m3）","0.071（扣参考值）",0.5,"是"]
[{"$nulls":5},"氨（mg/m3）",0.588,{"v":1,"d":"1.0"},"是"]
[null,null,"下风向边界点2#",null,null,"总悬浮颗粒物（mg/m3）","0.001（扣参考值）",0.5,"是"]
[{"$nulls":5},"氨（mg/m3）",0.226,{"v":1,"d":"1.0"},"是"]
[null,null,"下风向边界点1#","《恶臭污染物排放标准》（GB14554-93）表1 恶臭污染物厂界标准值",null,"硫化氢（mg/m3）","ND(0.0003)",0.06,"是"]
[{"$nulls":5},"甲硫醚（mg/m3）","ND(0.0004)",0.07,"是"]
[{"$nulls":5},"甲硫醇（mg/m3）","ND(0.0006)",0.007,"是"]
[{"$nulls":5},"苯乙烯（mg/m3）","ND(0.001)",{"v":5,"d":"5.0"},"是"]
[{"$nulls":5},"二甲二硫（mg/m3）","ND(0.0004)",0.06,"是"]
[null,null,"下风向边界点2#",null,null,"硫化氢（mg/m3）","ND(0.0003)",0.06,"是"]
[{"$nulls":5},"甲硫醚（mg/m3）","ND(0.0004)",0.07,"是"]
[{"$nulls":5},"甲硫醇（mg/m3）","ND(0.0006)",0.007,"是"]
[{"$nulls":5},"苯乙烯（mg/m3）","ND(0.001)",{"v":5,"d":"5.0"},"是"]
[{"$nulls":5},"二甲二硫（mg/m3）","ND(0.0004)",0.06,"是"]
[null,null,"下风向边界点1#",null,"2018-10-11","臭气浓度（无量纲）",13,20,"是"]
[null,null,"下风向边界点2#",null,null,"臭气浓度（无量纲）",12,20,"是"]
["黄埔区","广州恒运东区热力有限公司","4#75t/h锅炉处理后","《火电厂大气污染物排放标准》（GB13223-2011）表2大气污染物特别排放限值（燃煤锅炉）","2018-11-16","氮氧化物（mg/m3）",21,100,"是"]
[{"$nulls":5},"二氧化硫（mg/m3）",12,50,"是"]
[{"$nulls":5},"汞及其化合物(mg/m3)","ND(0.0025)",0.03,"是"]
[null,null,"4#75t/h锅炉烟囱排放口",null,null,"林格曼黑度（级）",0.5,1,"是"]
["南沙区","广州市梅山热电厂有限公司","停产"]
["黄埔区","广州瑞明电力股份有限公司","停产"]
["备注：","①结果中“ND”表示未检出，括号中数值为该项目检出限。"]
[null,"②表中*颗粒物（烟尘）均为实测浓度，按照GB/T 16157-1996修改单，采用本标准测定颗粒物浓度小于等于20 mg/m3时，测定结果表述为＜20 mg/m3,无法换算为基准含氧量状态下的基准排放浓度，故不做达标评价。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}