{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["采购明细"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"采购明细","index":0,"n_rows":43,"n_cols":4,"rows_kept":43,"merged":[[0,0,0,3]]}
["耗材需求"]
["序号","物品名称","参数","数量"]
[1,"氟化物","专用试剂50次/盒(适用于格林凯瑞G70pro）","1盒"]
[2,"硫化物","专用试剂100次/盒(适用于格林凯瑞G70pro）","1盒"]
[3,"铜","专用试剂50次/盒(适用于格林凯瑞G70pro）","2盒"]
[4,"氰化物","专用试剂100次/盒(适用于格林凯瑞G70pro）","1盒"]
[5,"总铬","专用试剂50次/盒(适用于格林凯瑞G70pro）","1盒"]
[6,"总磷","专用试剂100次/盒(适用于格林凯瑞G70pro）","1盒"]
[7,"六价铬","专用试剂50次/盒(适用于格林凯瑞G70pro）","1盒"]
[8,"氨氮","专用试剂100次/盒(适用于格林凯瑞G70pro）","1盒"]
[9,"挥发酚","专用试剂100次/盒(适用于格林凯瑞G70pro）","2盒"]
[10,"镍","专用试剂50次/盒","1盒"]
[11,"阴离子表面活性剂","专用试剂50次/盒(适用于格林凯瑞G70pro）","2盒"]
[12,"总氮","EPA专用试剂50次/盒(适用于格林凯瑞G70pro）","1盒"]
[13,"锌","专用试剂50次/盒(适用于格林凯瑞G70pro）","2盒"]
[14,"CODLR","专用预制试剂25次/盒(适用于格林凯瑞G70pro）","1盒"]
[15,"CODMHR","专用预制试剂25次/盒(适用于格林凯瑞G70pro）","1盒"]
[16,"COD（L）快速检测包","高锰酸盐氧化比色法，测试范围（0-5-10-13-20-50-100mg/L）","1盒"]
[17,"COD（H）快速检测包","高锰酸盐氧化比色法，测试范围（0-30-60-120-200-250mg/L）","1盒"]
[18,"氨氮（L）快速检测包","水杨酸比色法，测试范围（0-0.2-0.5-1-2-5-10mg/L）","1盒"]
[19,"总磷（L）快速检测包","钼酸铵比色法，测试范围（0-0.05-0.1-0.2-0.5-1mg/L）","1盒"]
[20,"总氮（L）快速检测包","水杨酸比色法，测试范围（0-1-2-5-10-20mg/L）","1盒"]
[21,"总（余）氯快速检测包","DPD比色法，测试范围（0.1-0.2-0.5-1-2-4-6.5-10mg/L）","1盒"]
[22,"挥发酚快速检测包","4-氨基安替比林比色法，测试范围（0-0.2-0.5-1-2-5-10mg/L）","1盒"]
[23,"阴离子表面活性剂快速检测包","溴百里酚蓝-氯代十六烷基吡啶比色法，测试范围（0-5-10-15-25-50mg/L）","1盒"]
[24,"色度快速检测包","铂钴标准比色法，测试范围（0-50-100-200-300-400-500mg/L）","1盒"]
[25,"金属总量（Cu、Zn、Mn、Ni、Cd）快速检测包","PAN比色法，测试范围（0.5-1-2-5-10-20mg/L）","1盒"]
[26,"总铜（L）快速检测包","锌试剂比色法，测试范围（0-0.1-0.3-0.5-0.7-1mg/L）","1盒"]
[27,"总镍（H）快速检测包","丁二酮肟比色法，测试范围（0-0.3-0.5-1-2-5mg/L）","1盒"]
[28,"总铬快速检测包","二苯碳酰二肼比色法，测试范围（0-0.1-0.2-0.5-1-2mg/L）","1盒"]
[29,"六价铬快速检测包","二苯碳酰二肼比色法，测试范围（0-0.1-0.2-0.5-1-2mg/L）","1盒"]
[30,"总锌快速检测包","双硫腙比色法，测试范围（0.2-0.5-1-2-5-10mg/L）","1盒"]
[31,"总镉快速检测包","双硫腙比色法，测试范围（0-0.1-0.2-0.5-1-2mg/L）","1盒"]
[32,"总汞快速检测包","双硫腙比色法，测试范围（0-0.2-0.5-1.0-2.0-5.0-10mg/L）","1盒"]
[33,"总砷快速检测包","钼酸铵比色法，测试范围（0-0.5-1-2-3-5mg/L）","1盒"]
[34,"氮气","含瓶8L","2瓶"]
[35,"甲烷","50×10-6mol/mol，氮气（平衡）,含瓶8L","1瓶"]
[36,"氮中氧气体标准物质","20.9%O2，N2余量，含瓶8L","1瓶"]
[37,"空气中甲烷气体标准物质","500×10-6mol/mol（以空气为配底）,含瓶8L","1瓶"]
[38,"空气中甲烷气体标准物质","1000×10-6mol/mol（以空气为配底）含瓶8L","1瓶"]
[39,"正己烷","4L，HPLC（Honeywell）","2瓶"]
[40,"一次性采样瓶","500mL，加厚HDPE无菌","500个"]
[41,"黄铜低量程气瓶减压阀","要求最低流量可达0.5L/min","1个"]