{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["试剂20250903"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"试剂20250903","index":0,"n_rows":81,"n_cols":7,"rows_kept":81,"merged":[[0,0,0,6]]}
["广州市生态环境局海珠环境监测站2025年实验室物资（第二批）采购明细"]
["序号","物品名称","参数","规格","单位","数量/瓶","备注"]
[1,"氢氧化钠","特优级,1000g/瓶",null,"瓶",2]
[2,"七水硫酸亚铁","AR",null,"瓶",2]
[3,"乳胶手套（小号）","无粉",null,"盒",5]
[4,"洗瓶机配套洗涤剂（套）","Cleaner 系列 ,5kg",null,"套",2,"酸性"]
[5,"氮-氮-二甲基对苯二胺盐酸盐","AR","25g","瓶",1]
[6,"乳胶手套（大号）","无粉",null,"盒",5]
[7,"乳胶手套（中号）","无粉",null,"盒",5]
[8,"洗耳球（大）","橡胶洗耳球90mL（大号）",null,"个",20]
[9,"洗耳球（中）","橡胶洗耳球60mL（中号）",null,"个",20]
[10,"洗耳球（小）","橡胶洗耳球30mL（小号）",null,"个",20,"用以吸1-2ml样品"]
[11,"带盖称量瓶（小）","内径约：36mm",null,"个",20]
[12,"带盖称量瓶（中）","内径约：52-53mm",null,"个",20]
[13,"擦镜纸","10*7.5cm，50张/本",null,"本",30]
[14,"小烧杯（10ml）","10mL",null,"个",20]
[15,"1ml单标移液管","A级,1ml",null,"支",20]
[16,"2ml单标移液管","A级,2ml",null,"支",10]
[17,"带分刻度纯水桶（刻度数值从下到上增大）\n（下部带水龙头（开关））","约25L",null,"个",1]
[18,"便携式溶解氧仪电极薄膜","PRO20",null,"套",2]
[19,"便携式pH计电极（上海三信）","适配三信pH计",null,"个",2]
[20,"哈希流动注射仪总磷滤光片","货号89880，波长880nm",null,"套",1]
[21,"噪声计三脚架","噪音计通用支架（展开1390mm，称重3kg，高度140cm，低高度55cm）",null,"个",2]
[22,"废水采样器（小铁桶）","不锈钢",null,"个",2]
[23,"户外应急手拉车","大号：超大560L，MAX聚拢后开+可折叠合金桌面，小号：越野款【双刹减震轮/承重400斤】+桌板",null,"辆",3,"1大2小（功能与参数和露营车类似）"]
[24,"个人应急防护包","适用于应急监测个人防护",null,"套",6,"含背包、防化服、全面防毒面具、防滑靴、防护手套、安全帽、反光衣、、强光手电筒、便携式头灯、雨衣、救生衣等"]
[25,"总氮标液","环保部标样所","20_mL","瓶",9]
[26,"一次性塑料采样瓶",null,null,"个",500]
[27,"总氮标样","环保部标样所","20_mL","瓶",9]
[28,"氟化物标液","环保部标样所","20_mL","瓶",8]
[29,"氟化物标样","环保部标样所","20_mL","瓶",9]
[30,"电导率标液","计量院","100_mL","瓶",4,"浓度147.6μS/cm"]
[31,"电导率标样","环保部标样所","20_mL","瓶",4]
[32,"六价铬标液","环保部标样所","20_mL","瓶",10]
[33,"六价铬标样","环保部标样所","20_mL","瓶",8]
[34,"总铬标液","环保部标样所","20_mL","瓶",3]
[35,"总铬标样","环保部标样所","20_mL","瓶",2]
[36,"氨氮标液","环保部标样所","20_mL","瓶",7]
[37,"氨氮标样","环保部标样所","20_mL","瓶",15]
[38,"硫化物标液","环保部标样所","20_mL","瓶",10]
[39,"硫化物标样","环保部标样所","20_mL","瓶",11]
[40,"挥发酚标液","环保部标样所","20_mL","瓶",6]
[41,"挥发酚标样","环保部标样所","20_mL","瓶",2]
[42,"总磷标液","环保部标样所","20_mL","瓶",5]
[43,"总磷标样","环保部标样所","20_mL","瓶",6]
[44,"总氰化物标液","计量院","50_mL","瓶",1]
[45,"四氯乙烯中的石油类标液","环保部标样所","20_mL","瓶",4]
[46,"铜标样","环保部标样所","20_mL","瓶",4]
[47,"锌标液","环保部标样所","20_mL","瓶",4]
[48,"草酸钠标液","环保部标样所","20_mL","瓶",4]
[49,"高锰酸钾容量分析用标准物质标液","环保部标样所","20_mL","瓶",6]
[50,"阴离子标液","环保部标样所","20_mL","瓶",7]
[51,"阴离子标样","环保部标样所","20_mL","瓶",5]
[52,"COD快速检测包","高锰酸盐氧化比色法，测试范围（0-5-10-13-20-50-100mg/L）",null,"盒",2]
[53,"COD快速检测包","高锰酸盐氧化比色法，测试范围（0-30-60-120-200-250mg/L）",null,"盒",2]
[54,"氨氮快速检测包","水杨酸比色法，测试范围（0-0.2-0.5-1-2-5-10mg/L）",null,"盒",2]
[55,"总磷快速检测包","钼酸铵比色法，测试范围（0-0.05-0.1-0.2-0.5-1mg/L）",null,"盒",2]
[56,"总氮快速检测包","水杨酸比色法，测试范围（0-1-2-5-10-20mg/L）",null,"盒",1]
[57,"总（余）氯快速检测包","DPD比色法，测试范围（0.1-0.2-0.5-1-2-4-6.5-10mg/L）",null,"盒",1]
[58,"色度快速检测包","铂钴标准比色法，测试范围（0-50-100-200-300-400-500mg/L）",null,"盒",1]
[59,"金属总量（Cu、Zn、Mn、Ni、Cd）快速检测包","PAN比色法，测试范围（0.5-1-2-5-10-20mg/L）",null,"盒",1]
[60,"总铜快速检测包","锌试剂比色法，测试范围（0-0.1-0.3-0.5-0.7-1mg/L）",null,"盒",1]
[61,"总镍快速检测包","丁二酮肟比色法，测试范围（0-0.3-0.5-1-2-5mg/L）",null,"盒",1]
[62,"总铬快速检测包","二苯碳酰二肼比色法，测试范围（0-0.1-0.2-0.5-1-2mg/L）",null,"盒",1]
[63,"六价铬快速检测包","二苯碳酰二肼比色法，测试范围（0-0.1-0.2-0.5-1-2mg/L）",null,"盒",1]
[64,"总锌快速检测包","双硫腙比色法，测试范围（0.2-0.5-1-2-5-10mg/L）",null,"盒",1]
[65,"总镉快速检测包","双硫腙比色法，测试范围（0-0.1-0.2-0.5-1-2mg/L）",null,"盒",1]
[66,"总汞快速检测包","双硫腙比色法，测试范围（0-0.2-0.5-1.0-2.0-5.0-10mg/L）",null,"盒",1]
[67,"总砷快速检测包","钼酸铵比色法，测试范围（0-0.5-1-2-3-5mg/L）",null,"盒",1]
[68,"标准气体浓度（包含以下7种）："]
[69,"#NO:1000mg/m3+N2平衡#","4L",null,"瓶",1]
[70,"#NO:500mg/m3+N2平衡#","4L",null,"瓶",1]
[71,"#NO:150mg/m3+N2平衡#","4L",null,"瓶",1]
[72,"#NO2:150mg/m3+N2平衡#","4L",null,"瓶",1]
[73,"#CO:100mg/m3+N2平衡#","4L",null,"瓶",1]
[74,"#SO2:150mg/m3+N2平衡#","4L",null,"瓶",1]
[75,"#O2:8%+N2平衡#","4L",null,"瓶",1]
[76,"实验室用气体（包含以下3种）："]
[77,"高纯氩气","40L",null,"瓶",3]
[78,"高纯氮气","40L",null,"瓶",1]
[79,"高纯乙炔","40L",null,"瓶",1]