{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["危险废物"],"not_rendered":{"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"危险废物","index":0,"n_rows":25,"n_cols":8,"rows_kept":25,"merged":[[1,0,1,7],[3,0,11,0],[3,1,11,1],[3,3,5,3],[3,4,5,4],[6,2,7,2],[6,3,11,3],[6,4,11,4],[8,2,9,2],[10,2,11,2],[12,0,19,0],[12,1,19,1],[12,3,13,3],[12,4,13,4],[14,2,15,2],[14,3,19,3],[14,4,19,4],[16,2,17,2],[18,2,19,2],[20,0,21,0],[20,1,21,1],[20,3,21,3]],"flags":["formulas_cached_only"]}
["附件3"]
["广州市2018年国控企业污染源（危废重点）监督性监测结果"]
["行政区","企业名称","监测点名称","执行标准名称","监测日期","监测项目名称（单位）","污染物浓度","标准限值"]
["白云区","广州永兴环保能源有限公司二分厂","焚烧炉渣1#","《生活垃圾焚烧污染控制标准》（GB18485-2014）表1生活垃圾焚烧炉主要技术性能指标","2018-10-19","热灼减率（%）",1.43,5]
[null,null,"焚烧炉渣2#",null,null,"热灼减率（%）",1.85,5]
[null,null,"焚烧炉渣3#",null,null,"热灼减率（%）",1.59,5]
[null,null,"厂界上风向监控点1#","《恶臭污染排放标准》（GB14554-93）二级新扩改建","2018-10-17","三甲胺（mg/m3）","ND(2.5×10-3)",0.08]
[{"$nulls":5},"二硫化碳（mg/m3）","ND(0.03)",3]
[null,null,"厂界上风向监控点2#",null,null,"三甲胺（mg/m3）","ND(2.5×10-3)",0.08]
[{"$nulls":5},"二硫化碳（mg/m3）","ND(0.03)",3]
[null,null,"厂界上风向监控点3#",null,null,"三甲胺（mg/m3）","ND(2.5×10-3)",0.08]
[{"$nulls":5},"二硫化碳（mg/m3）","ND(0.03)",3]
["白云区","广州永兴环保能源有限公司一分厂","焚烧炉渣1#","《生活垃圾焚烧污染控制标准》（GB18485-2014）表1生活垃圾焚烧炉主要技术性能指标","2018-10-19","热灼减率（%）",{"v":1.4,"d":"1.40"},5]
[null,null,"焚烧炉渣2#",null,null,"热灼减率（%）",1.62,5]
[null,null,"厂界上风向监控点1#","《恶臭污染排放标准》（GB14554-93）二级新扩改建","2018-10-17","三甲胺（mg/m3）","ND(2.5×10-3)",0.08]
[{"$nulls":5},"二硫化碳（mg/m3）","ND(0.03)",3]
[null,null,"厂界上风向监控点2#",null,null,"三甲胺（mg/m3）","ND(2.5×10-3)",0.08]
[{"$nulls":5},"二硫化碳（mg/m3）","ND(0.03)",3]
[null,null,"厂界上风向监控点3#",null,null,"三甲胺（mg/m3）","ND(2.5×10-3)",0.08]
[{"$nulls":5},"二硫化碳（mg/m3）","ND(0.03)",3]
["南沙区","广州绿由工业弃置废物回收处理有限公司","15t/h焚烧炉处理后采样口","《危险废物焚烧污染控制标准》（GB18484－2001）","2018-10-22","氯化氢（mg/m3）",1.4,60]
[null,null,"焚烧炉渣",null,"2018-10-23","热灼减率（%）",3.58,"＜5"]
["备注","1、广州绿由工业弃置废物回收处理有限公司的氯化氢和热灼减率数据分别由广州华清环境监测有限公司和中国广州分析测试中心提供。"]
[null,"2、广州永兴环保能源有限公司一分厂和二分厂的热灼减率数据由中国广州分析测试中心提供。"]
[null,"3、厂界无组织排放中的三甲胺和二硫化碳数据由广州华清环境监测有限公司提供。"]