{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["污水厂","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"污水厂","index":0,"n_rows":506,"n_cols":9,"rows_kept":506,"merged":[[0,0,0,7],[1,0,1,8],[3,0,40,0],[3,1,40,1],[3,2,21,2],[3,3,21,3],[3,4,21,4],[22,2,40,2],[22,3,40,3],[22,4,40,4],[41,0,97,0],[41,1,97,1],[41,2,59,2],[41,3,59,3],[41,4,59,4],[60,2,78,2],[60,3,78,3],[60,4,78,4],[79,2,97,2],[79,3,97,3],[79,4,97,4],[98,0,116,0],[98,1,116,1],[98,2,116,2],[98,3,116,3],[98,4,116,4],[117,0,135,0],[117,1,135,1],[117,2,135,2],[117,3,135,3],[117,4,135,4],[136,0,154,0],[136,1,154,1],[136,2,154,2],[136,3,154,3],[136,4,154,4],[155,0,173,0],[155,1,173,1],[155,2,173,2],[155,3,173,3],[155,4,173,4],[174,0,192,0],[174,1,192,1],[174,2,192,2],[174,3,192,3],[174,4,192,4],[193,0,211,0],[193,1,211,1],[193,2,211,2],[193,3,211,3],[193,4,211,4],[212,0,230,0],[212,1,230,1],[212,2,230,2],[212,3,230,3],[212,4,230,4],[231,0,249,0],[231,1,249,1],[231,2,249,2],[231,3,249,3],[231,4,249,4],[250,0,268,0],[250,1,268,1],[250,2,268,2],[250,3,268,3],[250,4,268,4],[269,0,287,0],[269,1,287,1],[269,2,287,2],[269,3,287,3],[269,4,287,4],[288,0,306,0],[288,1,306,1],[288,2,306,2],[288,3,306,3],[288,4,306,4],[307,0,325,0],[307,1,325,1],[307,2,325,2],[307,3,325,3],[307,4,325,4],[326,0,344,0],[326,1,344,1],[326,2,344,2],[326,3,344,3],[326,4,344,4],[345,0,369,0],[345,1,369,1],[345,2,369,2],[345,3,369,3],[345,4,369,4],[370,0,388,0],[370,1,388,1],[370,2,388,2],[370,3,388,3],[370,4,388,4],[389,0,407,0],[389,1,407,1],[389,2,407,2],[389,3,407,3],[389,4,407,4],[408,0,426,0],[408,1,426,1],[408,2,426,2],[408,3,426,3],[408,4,426,4],[427,0,445,0],[427,1,445,1],[427,2,445,2],[427,3,445,3],[427,4,445,4],[446,0,464,0],[446,1,464,1],[446,2,464,2],[446,3,464,3],[446,4,464,4],[465,0,483,0],[465,1,483,1],[465,2,483,2],[465,3,483,3],[465,4,483,4],[484,0,502,0],[484,1,502,1],[484,2,502,2],[484,3,502,3],[484,4,502,4]],"flags":["formulas_cached_only"]}
["附件1"]
["广州市2018年国控企业污染源（污水处理厂）监督性监测结果（第4季度）"]
["行政区","企业名称","监测点位","监测日期","执行标准名称","监测项目名称(单位)","污染物浓度","标准限值","是否达标"]
["海珠区","广州市沥滘污水处理厂","一期出水口","2018-10-16","广东省《水污染物排放限值》(DB44/26-2001）第二时段二级标准","pH值(无量纲)",7.22,"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)",0.221,15,"是"]
[{"$nulls":5},"动植物油(mg/L）","ND(0.04)",15,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10","/","/"]
[{"$nulls":5},"化学需氧量(mg/L）",15,60,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.5,"是"]
[{"$nulls":5},"色度（倍）",4,60,"是"]
[{"$nulls":5},"石油类(mg/L）",0.07,8,"是"]
[{"$nulls":5},"烷基汞(mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",2.9,30,"是"]
[{"$nulls":5},"悬浮物(mg/L）",12,30,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）","ND(0.05)",10,"是"]
[{"$nulls":5},"总氮(mg/L）",12.1,"/","/"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.1,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",1.5,"是"]
[{"$nulls":5},"总汞(mg/L）","ND(9×10-6)",0.05,"是"]
[{"$nulls":5},"总磷(mg/L）",0.19,{"v":1,"d":"1.0"},"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.5,"是"]
[null,null,"二期出水口","2018-10-16","《城镇污水处理厂污染物排放标准》（GB18918-2002）一级B标准","pH值(无量纲)",7.17,"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)",0.243,8,"是"]
[{"$nulls":5},"动植物油(mg/L）","ND(0.04)",3,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10",10000,"是"]
[{"$nulls":5},"化学需氧量(mg/L）",15,60,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.05,"是"]
[{"$nulls":5},"色度（倍）",4,30,"是"]
[{"$nulls":5},"石油类(mg/L）",0.05,3,"是"]
[{"$nulls":5},"烷基汞(mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",3.2,20,"是"]
[{"$nulls":5},"悬浮物(mg/L）",16,20,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）",0.06,1,"是"]
[{"$nulls":5},"总氮(mg/L）",11.1,20,"是"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.01,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",0.1,"是"]
[{"$nulls":5},"总汞(mg/L）","ND(9×10-6)",0.001,"是"]
[{"$nulls":5},"总磷(mg/L）",0.27,1,"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",0.1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.1,"是"]
["天河区","广州市猎德污水处理厂","一、二期出水口","2018-10-16","《城镇污水处理厂污染物排放标准》（GB18918-2002）一级B标准+广东省《水污染物排放限值》(DB44/26-2001）第二时段一级标准","pH值(无量纲)",7.08,"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)",0.392,8,"是"]
[{"$nulls":5},"动植物油(mg/L）","ND(0.04)",3,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10",10000,"是"]
[{"$nulls":5},"化学需氧量(mg/L）",11,40,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.05,"是"]
[{"$nulls":5},"色度（倍）",4,30,"是"]
[{"$nulls":5},"石油类(mg/L）",0.06,3,"是"]
[{"$nulls":5},"烷基汞(mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",2.6,20,"是"]
[{"$nulls":5},"悬浮物(mg/L）",8,20,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）",0.05,1,"是"]
[{"$nulls":5},"总氮(mg/L）",9.91,20,"是"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.01,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",0.1,"是"]
[{"$nulls":5},"总汞(mg/L）","3.0×10-5",0.001,"是"]
[{"$nulls":5},"总磷(mg/L）",0.15,0.5,"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",0.1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.1,"是"]
[null,null,"三期出水口","2018-10-16","《城镇污水处理厂污染物排放标准》（GB18918-2002）一级B标准+广东省《水污染物排放限值》(DB44/26-2001）第二时段一级标准","pH值(无量纲)",7.12,"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)",0.185,8,"是"]
[{"$nulls":5},"动植物油(mg/L）","ND(0.04)",3,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10",10000,"是"]
[{"$nulls":5},"化学需氧量(mg/L）",13,40,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.05,"是"]
[{"$nulls":5},"色度（倍）",4,30,"是"]
[{"$nulls":5},"石油类(mg/L）",0.08,3,"是"]
[{"$nulls":5},"烷基汞(mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",2.9,20,"是"]
[{"$nulls":5},"悬浮物(mg/L）",8,20,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）","ND(0.05)",1,"是"]
[{"$nulls":5},"总氮(mg/L）",9.38,20,"是"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.01,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",0.1,"是"]
[{"$nulls":5},"总汞(mg/L）","3.6×10-5",0.001,"是"]
[{"$nulls":5},"总磷(mg/L）",0.11,0.5,"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",0.1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.1,"是"]
[null,null,"四期出水口","2018-10-16","《城镇污水处理厂污染物排放标准》（GB18918-2002）一级A标准+广东省《水污染物排放限值》(DB44/26-2001）第二时段一级标准","pH值(无量纲)",7.15,"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)",0.108,5,"是"]
[{"$nulls":5},"动植物油(mg/L）","ND(0.04)",1,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10",1000,"是"]
[{"$nulls":5},"化学需氧量(mg/L）",10,40,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.05,"是"]
[{"$nulls":5},"色度（倍）",4,30,"是"]
[{"$nulls":5},"石油类(mg/L）",0.06,1,"是"]
[{"$nulls":5},"烷基汞(mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",2.5,10,"是"]
[{"$nulls":5},"悬浮物(mg/L）",9,10,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）","ND(0.05)",0.5,"是"]
[{"$nulls":5},"总氮(mg/L）",6.06,15,"是"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.01,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",0.1,"是"]
[{"$nulls":5},"总汞(mg/L）","7.4×10-5",0.001,"是"]
[{"$nulls":5},"总磷(mg/L）",{"v":0.1,"d":"0.10"},0.5,"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",0.1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.1,"是"]
["黄埔区","广州开发区萝岗区水质净化管理中心（西区水质净化厂）","出水口","2018-10-19","《城镇污水处理厂污染物排放标准》（GB18918-2002）一级B标准+《水污染物排放限值》(DB44/26-2001）第二时段一级标准","pH值(无量纲)",7.21,"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)",0.116,8,"是"]
[{"$nulls":5},"动植物油(mg/L）","ND(0.04)",3,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10",10000,"是"]
[{"$nulls":5},"化学需氧量(mg/L）",5,40,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.05,"是"]
[{"$nulls":5},"色度（倍）",4,30,"是"]
[{"$nulls":5},"石油类(mg/L）",0.07,3,"是"]
[{"$nulls":5},"烷基汞(mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",1.4,20,"是"]
[{"$nulls":5},"悬浮物(mg/L）",9,20,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）","ND(0.05)",1,"是"]
[{"$nulls":5},"总氮(mg/L）",4.36,20,"是"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.01,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",0.1,"是"]
[{"$nulls":5},"总汞(mg/L）","2.8×10-5",0.001,"是"]
[{"$nulls":5},"总磷(mg/L）",0.12,0.5,"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",0.1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.1,"是"]
["黄埔区","广州开发区萝岗区水质净化管理中心（东区水质净化厂）","出水口","2018-10-16","《城镇污水处理厂污染物排放标准》（GB18918-2002）一级B标准","pH值(无量纲)",7.05,"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)","ND(0.025)",8,"是"]
[{"$nulls":5},"动植物油(mg/L）","ND(0.04)",3,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10",10000,"是"]
[{"$nulls":5},"化学需氧量(mg/L）",5,60,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.05,"是"]
[{"$nulls":5},"色度（倍）",4,30,"是"]
[{"$nulls":5},"石油类(mg/L）",0.05,3,"是"]
[{"$nulls":5},"烷基汞(mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",1.2,20,"是"]
[{"$nulls":5},"悬浮物(mg/L）",8,20,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）","ND(0.05)",1,"是"]
[{"$nulls":5},"总氮(mg/L）",1.81,20,"是"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.01,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",0.1,"是"]
[{"$nulls":5},"总汞(mg/L）","7.0×10-5",0.001,"是"]
[{"$nulls":5},"总磷(mg/L）",0.03,1,"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",0.1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.1,"是"]
["花都区","广州白云国际机场股份有限公司（机场污水处理站）","出水口","2018-10-17","《城镇污水处理厂污染物排放标准》（GB18918-2002）一级B标准+广东省《水污染物排放限值》(DB44/26-2001）第二时段一级标准","pH值(无量纲)",7.18,"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)",0.356,8,"是"]
[{"$nulls":5},"动植物油(mg/L）","ND(0.04)",3,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10",10000,"是"]
[{"$nulls":5},"化学需氧量(mg/L）",4,40,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.05,"是"]
[{"$nulls":5},"色度（倍）",4,30,"是"]
[{"$nulls":5},"石油类(mg/L）",0.07,3,"是"]
[{"$nulls":5},"烷基汞(mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",1.3,20,"是"]
[{"$nulls":5},"悬浮物(mg/L）",8,20,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）","ND(0.05)",1,"是"]
[{"$nulls":5},"总氮(mg/L）",3.12,20,"是"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.01,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",0.1,"是"]
[{"$nulls":5},"总汞(mg/L）","7.4×10-5",0.001,"是"]
[{"$nulls":5},"总磷(mg/L）",0.08,0.5,"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",0.1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.1,"是"]
["白云区","东华工业区生活污水处理站","出水口","2018-10-17","广东省《水污染物排放限值》(DB44/26-2001）第二时段二级标准","pH值(无量纲)",7.21,"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)",13.2,15,"是"]
[{"$nulls":5},"动植物油(mg/L）",0.07,15,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）",10,"/","/"]
[{"$nulls":5},"化学需氧量(mg/L）",14,110,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.5,"是"]
[{"$nulls":5},"色度（倍）",4,60,"是"]
[{"$nulls":5},"石油类(mg/L）","ND(0.04)",8,"是"]
[{"$nulls":5},"烷基汞(mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",4.3,30,"是"]
[{"$nulls":5},"悬浮物(mg/L）",9,100,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）","ND(0.05)",10,"是"]
[{"$nulls":5},"总氮(mg/L）",18.9,"/","/"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.1,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",1.5,"是"]
[{"$nulls":5},"总汞(mg/L）","5.4×10-5",0.05,"是"]
[{"$nulls":5},"总磷(mg/L）",0.04,{"v":1,"d":"1.0"},"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.5,"是"]
["黄埔区","广州市污水治理有限责任公司（大沙地污水处理厂）","出水口","2018-10-18","广东省《水污染物排放限值》(DB44/26-2001）第二时段二级标准","pH值（无量纲）",7.14,"6～9","是"]
[{"$nulls":5},"氨氮（mg/L）",0.166,15,"是"]
[{"$nulls":5},"动植物油（mg/L）","ND(0.04)",15,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10","/","/"]
[{"$nulls":5},"化学需氧量（mg/L）",9,60,"是"]
[{"$nulls":5},"六价铬（mg/L）","ND(0.004)",0.5,"是"]
[{"$nulls":5},"色度(倍)",4,60,"是"]
[{"$nulls":5},"石油类（mg/L）",0.07,8,"是"]
[{"$nulls":5},"烷基汞（mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量（mg/L）",2.6,30,"是"]
[{"$nulls":5},"悬浮物（mg/L）",8,30,"是"]
[{"$nulls":5},"阴离子表面活性剂（mg/L）","ND(0.05)",10,"是"]
[{"$nulls":5},"总氮（mg/L）",8.54,"/","/"]
[{"$nulls":5},"总镉（mg/L）","ND(0.003)",0.1,"是"]
[{"$nulls":5},"总铬（mg/L）","ND(0.01)",1.5,"是"]
[{"$nulls":5},"总汞（mg/L）","1.8×10-5",0.05,"是"]
[{"$nulls":5},"总磷（mg/L）",0.23,{"v":1,"d":"1.0"},"是"]
[{"$nulls":5},"总铅（mg/L）","ND(0.05)",1,"是"]
[{"$nulls":5},"总砷（mg/L）","ND(0.01)",0.5,"是"]
["花都区","广州中业污水处理有限公司（花都区新华污水处理厂一、二期）","总排放口","2018-10-22","《城镇污水处理厂污染物排放标准》（GB18918-2002）一级A标准+广东省《水污染物排放限值》(DB44/26-2001）第二时段一级标准","pH值(无量纲)",7.08,"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)",0.077,5,"是"]
[{"$nulls":5},"动植物油(mg/L）","ND(0.04)",1,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10",1000,"是"]
[{"$nulls":5},"化学需氧量(mg/L）",5,40,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.05,"是"]
[{"$nulls":5},"色度（倍）",4,30,"是"]
[{"$nulls":5},"石油类(mg/L）",0.06,1,"是"]
[{"$nulls":5},"烷基汞(mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",1.7,10,"是"]
[{"$nulls":5},"悬浮物(mg/L）",9,10,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）",0.06,0.5,"是"]
[{"$nulls":5},"总氮(mg/L）",6.46,15,"是"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.01,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",0.1,"是"]
[{"$nulls":5},"总汞(mg/L）","1.10×10-4",0.001,"是"]
[{"$nulls":5},"总磷(mg/L）",0.12,0.5,"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",0.1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.1,"是"]
["黄埔区","广州开发区萝岗区水质净化管理中心（永和水质净化厂）","出水口","2018-10-18","《城镇污水处理厂污染物排放标准》（GB18918-2002）一级B标准+《水污染物排放限值》(DB44/26-2001）第二时段一级标准","pH值(无量纲)",7.03,"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)",0.066,8,"是"]
[{"$nulls":5},"动植物油(mg/L）","ND(0.04)",3,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10",10000,"是"]
[{"$nulls":5},"化学需氧量(mg/L）",5,40,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.05,"是"]
[{"$nulls":5},"色度（倍）",4,30,"是"]
[{"$nulls":5},"石油类(mg/L）",0.05,3,"是"]
[{"$nulls":5},"烷基汞(mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",1.3,20,"是"]
[{"$nulls":5},"悬浮物(mg/L）",9,20,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）","ND(0.05)",1,"是"]
[{"$nulls":5},"总氮(mg/L）",1.91,20,"是"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.01,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",0.1,"是"]
[{"$nulls":5},"总汞(mg/L）","1.8×10-5",0.001,"是"]
[{"$nulls":5},"总磷(mg/L）",0.06,0.5,"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",0.1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.1,"是"]
["花都区","广州市新狮水务有限公司（狮岭污水处理厂一期）","出水口","2018-10-17","《城镇污水处理厂污染物排放标准》（GB18918-2002）一级B标准+《水污染物排放限值》(DB44/26-2001）第二时段一级标准","pH值(无量纲)",7.15,"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)",0.047,8,"是"]
[{"$nulls":5},"动植物油(mg/L）",0.07,3,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10",10000,"是"]
[{"$nulls":5},"化学需氧量(mg/L）",10,40,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.05,"是"]
[{"$nulls":5},"色度（倍）",4,30,"是"]
[{"$nulls":5},"石油类(mg/L）","ND(0.04)",3,"是"]
[{"$nulls":5},"烷基汞(mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",2.1,20,"是"]
[{"$nulls":5},"悬浮物(mg/L）",8,20,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）","ND(0.05)",1,"是"]
[{"$nulls":5},"总氮(mg/L）",{"v":5.5,"d":"5.50"},20,"是"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.01,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",0.1,"是"]
[{"$nulls":5},"总汞(mg/L）","5.1×10-5",0.001,"是"]
[{"$nulls":5},"总磷(mg/L）",0.05,0.5,"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",0.1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.1,"是"]
["增城区","广州科美环保实业有限公司","出水口","2018-10-16","广东省《水污染物排放限值》(DB44/26-2001）第二时段一级标准+《城镇污水处理厂污染物排放标准》（GB18918-2002）一级标准B标准","pH值（无量纲）",7.14,"6～9","是"]
[{"$nulls":5},"氨氮（mg/L）",0.041,8,"是"]
[{"$nulls":5},"动植物油（mg/L）",0.05,3,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10",10000,"是"]
[{"$nulls":5},"化学需氧量（mg/L）",5,40,"是"]
[{"$nulls":5},"六价铬（mg/L）","ND(0.004)",0.05,"是"]
[{"$nulls":5},"色度（倍）",4,30,"是"]
[{"$nulls":5},"石油类（mg/L）","ND(0.04)",3,"是"]
[{"$nulls":5},"烷基汞（mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量（mg/L）",1.3,20,"是"]
[{"$nulls":5},"悬浮物（mg/L）",12,20,"是"]
[{"$nulls":5},"阴离子表面活性剂（mg/L）",0.05,1,"是"]
[{"$nulls":5},"总氮（mg/L）",4.47,20,"是"]
[{"$nulls":5},"总镉（mg/L）","ND(0.003)",0.01,"是"]
[{"$nulls":5},"总铬（mg/L）","ND(0.01)",0.1,"是"]
[{"$nulls":5},"总汞（mg/L）","8.3×10-5",0.001,"是"]
[{"$nulls":5},"总磷（mg/L）",0.28,0.5,"是"]
[{"$nulls":5},"总铅（mg/L）","ND(0.05)",0.1,"是"]
[{"$nulls":5},"总砷（mg/L）","ND(0.01)",0.1,"是"]
["白云区","广州市净水有限公司龙归分公司","出水口","2018-10-19","《城镇污水处理厂污染物排放标准》（GB18918-2002）一级A标准+广东省《水污染物排放限值》(DB44/26-2001）第二时段一级标准","pH值(无量纲)",6.57,"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)",0.127,5,"是"]
[{"$nulls":5},"动植物油(mg/L）","ND(0.04)",1,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10",1000,"是"]
[{"$nulls":5},"化学需氧量(mg/L）",7,40,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.05,"是"]
[{"$nulls":5},"色度（倍）",4,30,"是"]
[{"$nulls":5},"石油类(mg/L）",0.07,1,"是"]
[{"$nulls":5},"烷基汞(mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",1.8,10,"是"]
[{"$nulls":5},"悬浮物(mg/L）",8,10,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）","ND(0.05)",0.5,"是"]
[{"$nulls":5},"总氮(mg/L）",8.28,15,"是"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.01,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",0.1,"是"]
[{"$nulls":5},"总汞(mg/L）","4.0×10-5",0.001,"是"]
[{"$nulls":5},"总磷(mg/L）",0.25,0.5,"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",0.1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.1,"是"]
["白云区","广州市净水有限公司竹料分公司","出水口","2018-10-15","《城镇污水处理厂污染物排放标准》（GB18918-2002）一级A标准+广东省《水污染物排放限值》(DB44/26-2001）第二时段一级标准","pH值(无量纲)",7.16,"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)",{"v":0.03,"d":"0.030"},5,"是"]
[{"$nulls":5},"动植物油(mg/L）",0.04,1,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10",1000,"是"]
[{"$nulls":5},"化学需氧量(mg/L）",6,40,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.05,"是"]
[{"$nulls":5},"色度（倍）",4,30,"是"]
[{"$nulls":5},"石油类(mg/L）","ND(0.04)",1,"是"]
[{"$nulls":5},"烷基汞(mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",1.3,10,"是"]
[{"$nulls":5},"悬浮物(mg/L）",9,10,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）","ND(0.05)",0.5,"是"]
[{"$nulls":5},"总氮(mg/L）",6.15,15,"是"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.01,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",0.1,"是"]
[{"$nulls":5},"总汞(mg/L）","4.0×10-5",0.001,"是"]
[{"$nulls":5},"总磷(mg/L）",0.04,0.5,"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",0.1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.1,"是"]
["白云区","广州市净水有限公司京溪分公司","出水口","2018-10-15","《城镇污水处理厂污染物排放标准》（GB18918-2002）一级A标准+广东省《水污染物排放限值》(DB44/26-2001）第二时段一级标准","pH值(无量纲)",7.13,"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)",0.094,5,"是"]
[{"$nulls":5},"动植物油(mg/L）","ND(0.04)",1,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10",1000,"是"]
[{"$nulls":5},"化学需氧量(mg/L）",10,40,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.05,"是"]
[{"$nulls":5},"色度（倍）",4,30,"是"]
[{"$nulls":5},"石油类(mg/L）","ND(0.04)",1,"是"]
[{"$nulls":5},"烷基汞(mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",2.2,10,"是"]
[{"$nulls":5},"悬浮物(mg/L）",8,10,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）","ND(0.05)",0.5,"是"]
[{"$nulls":5},"总氮(mg/L）",8.37,15,"是"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.01,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",0.1,"是"]
[{"$nulls":5},"总汞(mg/L）","ND(9×10-6)",0.001,"是"]
[{"$nulls":5},"总磷(mg/L）",0.18,0.5,"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",0.1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.1,"是"]
["南沙区","广州市番禺污水治理有限公司（大岗污水处理厂）","出水口","2018-10-17","《城镇污水处理厂污染物排放标准》（GB18918-2002）一级B标准+《水污染物排放限值》(DB44/26-2001）第二时段一级标准","pH值(无量纲)",7.05,"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)",0.218,8,"是"]
[{"$nulls":5},"动植物油(mg/L）",0.08,3,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10",10000,"是"]
[{"$nulls":5},"化学需氧量(mg/L）",8,40,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.05,"是"]
[{"$nulls":5},"色度（倍）",4,30,"是"]
[{"$nulls":5},"石油类(mg/L）","ND(0.04)",3,"是"]
[{"$nulls":5},"烷基汞(mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",2.1,20,"是"]
[{"$nulls":5},"悬浮物(mg/L）",9,20,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）","ND(0.05)",1,"是"]
[{"$nulls":5},"总氮(mg/L）",2.34,20,"是"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.01,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",0.1,"是"]
[{"$nulls":5},"总汞(mg/L）","4.5×10-5",0.001,"是"]
[{"$nulls":5},"总磷(mg/L）",0.19,0.5,"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",0.1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.1,"是"]
["南沙区","广州市番禺东涌工业污水处理有限公司","出水口","2018-10-18","《纺织染整工业水污染物排放标准》（GB4287-2012）+广东省《水污染物排放限值》(DB44/26-2001）第二时段一级标准","pH(无量纲)",{"v":7.2,"d":"7.20"},"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)",0.166,10,"是"]
[{"$nulls":5},"苯胺类(mg/L)",0.13,{"v":1,"d":"1.0"},"是"]
[{"$nulls":5},"动植物油(mg/L）","ND(0.04)",10,"是"]
[{"$nulls":5},"二氧化氯(mg/L)",0.14,0.5,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","4.7×102","/","/"]
[{"$nulls":5},"化学需氧量(mg/L）",13,80,"是"]
[{"$nulls":5},"挥发酚(mg/L)","ND(0.01)",0.3,"是"]
[{"$nulls":5},"硫化物(mg/L）","ND(0.005)",0.5,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.5,"是"]
[{"$nulls":5},"色度（倍）",4,40,"是"]
[{"$nulls":5},"石油类(mg/L）",0.06,5,"是"]
[{"$nulls":5},"烷基汞(mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",3.2,20,"是"]
[{"$nulls":5},"悬浮物(mg/L）",9,50,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）",0.06,5,"是"]
[{"$nulls":5},"总氮(mg/L）",7.72,15,"是"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.1,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",1.5,"是"]
[{"$nulls":5},"总汞(mg/L）","ND(9×10-6)",0.05,"是"]
[{"$nulls":5},"总磷(mg/L）",0.08,0.5,"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.5,"是"]
[{"$nulls":5},"总锑(mg/L）","2.8×10-3",0.1,"是"]
[{"$nulls":5},"总铜(mg/L)","ND(0.01)",0.5,"是"]
["黄埔区","广州开发区萝岗区水质净化管理中心（九龙水质净化一厂）","出水口","2018-10-19","《城镇污水处理厂污染物排放标准》（GB18918-2002）一级B标准","pH值(无量纲)",7.13,"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)","ND(0.025)",8,"是"]
[{"$nulls":5},"动植物油(mg/L）",0.44,3,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）",60,10000,"是"]
[{"$nulls":5},"化学需氧量(mg/L）",5,60,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.05,"是"]
[{"$nulls":5},"色度（倍）",4,30,"是"]
[{"$nulls":5},"石油类(mg/L）",0.15,3,"是"]
[{"$nulls":5},"烷基汞(mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",1.6,20,"是"]
[{"$nulls":5},"悬浮物(mg/L）",8,20,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）","ND(0.05)",1,"是"]
[{"$nulls":5},"总氮(mg/L）",3.74,20,"是"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.01,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",0.1,"是"]
[{"$nulls":5},"总汞(mg/L）","5.3×10-5",0.001,"是"]
[{"$nulls":5},"总磷(mg/L）","ND(0.01)",1,"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",0.1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.1,"是"]
["南沙区","中信环境水务（广州）有限公司","出水口","2018-10-17","广东省《水污染物排放限值》(DB44/26-2001）第二时段一级标准","pH值(无量纲)",7.08,"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)",0.229,10,"是"]
[{"$nulls":5},"动植物油(mg/L）","ND(0.04)",10,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10","/","/"]
[{"$nulls":5},"化学需氧量(mg/L）",16,40,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.5,"是"]
[{"$nulls":5},"色度（倍）",4,40,"是"]
[{"$nulls":5},"石油类(mg/L）",0.07,5,"是"]
[{"$nulls":5},"烷基汞(mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",3.3,20,"是"]
[{"$nulls":5},"悬浮物(mg/L）",8,20,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）","ND(0.05)",5,"是"]
[{"$nulls":5},"总氮(mg/L）",1.18,"/","/"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.1,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",1.5,"是"]
[{"$nulls":5},"总汞(mg/L）","4.0×10-5",0.05,"是"]
[{"$nulls":5},"总磷(mg/L）",0.16,0.5,"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.5,"是"]
["番禺区","广州市番禺污水治理有限公司（大石污水处理厂）","出水口","2018-10-22","《城镇污水处理厂污染物排放标准》（GB18918-2002）一级A标准+广东省《水污染物排放限值》(DB44/26-2001）第二时段一级标准","pH值(无量纲)",7.16,"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)",1.02,5,"是"]
[{"$nulls":5},"动植物油(mg/L）","ND(0.04)",1,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10",1000,"是"]
[{"$nulls":5},"化学需氧量(mg/L）",7,40,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.05,"是"]
[{"$nulls":5},"色度（倍）",4,30,"是"]
[{"$nulls":5},"石油类(mg/L）",0.07,1,"是"]
[{"$nulls":5},"烷基汞(mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",2.3,10,"是"]
[{"$nulls":5},"悬浮物(mg/L）",8,10,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）","ND(0.05)",0.5,"是"]
[{"$nulls":5},"总氮(mg/L）",3.94,15,"是"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.01,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",0.1,"是"]
[{"$nulls":5},"总汞(mg/L）","3.7×10-5",0.001,"是"]
[{"$nulls":5},"总磷(mg/L）",0.22,0.5,"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",0.1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.1,"是"]
["增城区","广州市新明润水质净化有限公司","出水口","2018-10-16","《城镇污水处理厂污染物排放标准》（GB18918-2002）一级A标准+广东省《水污染物排放限值》(DB44/26-2001）第二时段一级标准","pH值（无量纲）",7.21,"6～9","是"]
[{"$nulls":5},"氨氮（mg/L）","ND(0.025)",5,"是"]
[{"$nulls":5},"动植物油（mg/L）","ND(0.04)",1,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10",1000,"是"]
[{"$nulls":5},"化学需氧量（mg/L）",8,40,"是"]
[{"$nulls":5},"六价铬（mg/L）","ND(0.004)",0.05,"是"]
[{"$nulls":5},"色度(倍)",4,30,"是"]
[{"$nulls":5},"石油类（mg/L）",0.05,1,"是"]
[{"$nulls":5},"烷基汞（ng/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量（mg/L）",1.7,10,"是"]
[{"$nulls":5},"悬浮物（mg/L）",8,10,"是"]
[{"$nulls":5},"阴离子表面活性剂（mg/L）",0.11,0.5,"是"]
[{"$nulls":5},"总氮（mg/L）",{"v":12,"d":"12.0"},15,"是"]
[{"$nulls":5},"总镉（mg/L）","ND(0.003)",0.01,"是"]
[{"$nulls":5},"总铬（mg/L）","ND(0.01)",0.1,"是"]
[{"$nulls":5},"总汞（mg/L）","5.7×10-5",0.001,"是"]
[{"$nulls":5},"总磷（mg/L）",0.38,0.5,"是"]
[{"$nulls":5},"总铅（mg/L）","ND(0.05)",0.1,"是"]
[{"$nulls":5},"总砷（mg/L）","ND(0.01)",0.1,"是"]
["增城区","广州海滔环保科技有限公司","出水口","2018-10-10","《城镇污水处理厂污染物排放标准》（GB18918-2002）一级A标准+广东省《水污染物排放限值》(DB44/26-2001）第二时段一级标准","pH值(无量纲)",7.07,"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)",0.094,5,"是"]
[{"$nulls":5},"动植物油(mg/L）","ND(0.04)",1,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10",1000,"是"]
[{"$nulls":5},"化学需氧量(mg/L）",5,40,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.05,"是"]
[{"$nulls":5},"色度（倍）",16,30,"是"]
[{"$nulls":5},"石油类(mg/L）","ND(0.04)",1,"是"]
[{"$nulls":5},"烷基汞(mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",1.4,10,"是"]
[{"$nulls":5},"悬浮物(mg/L）",8,10,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）",0.07,0.5,"是"]
[{"$nulls":5},"总氮(mg/L）",11.3,15,"是"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.01,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",0.1,"是"]
[{"$nulls":5},"总汞(mg/L）","1.48×10-4",0.001,"是"]
[{"$nulls":5},"总磷(mg/L）",0.25,0.5,"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",0.1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.1,"是"]
["增城区","广州骏鹏投资有限公司","出水口","2018-10-15","广东省《水污染物排放限值》(DB44/26-2001）第二时段一级标准+《城镇污水处理厂污染物排放标准》（GB18918-2002）一级A标准","pH值(无量纲)",7.07,"6～9","是"]
[{"$nulls":5},"氨氮(mg/L)",0.033,5,"是"]
[{"$nulls":5},"动植物油(mg/L）",0.05,{"v":1,"d":"1.0"},"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10",1000,"是"]
[{"$nulls":5},"化学需氧量(mg/L）",6,40,"是"]
[{"$nulls":5},"六价铬(mg/L）","ND(0.004)",0.05,"是"]
[{"$nulls":5},"色度（倍）",4,30,"是"]
[{"$nulls":5},"石油类(mg/L）","ND(0.04)",{"v":1,"d":"1.0"},"是"]
[{"$nulls":5},"烷基汞（mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量(mg/L）",1.4,10,"是"]
[{"$nulls":5},"悬浮物(mg/L）",8,10,"是"]
[{"$nulls":5},"阴离子表面活性剂(mg/L）",0.06,0.5,"是"]
[{"$nulls":5},"总氮(mg/L）",7.59,15,"是"]
[{"$nulls":5},"总镉(mg/L）","ND(0.003)",0.01,"是"]
[{"$nulls":5},"总铬(mg/L）","ND(0.01)",0.1,"是"]
[{"$nulls":5},"总汞（mg/L）","6.2×10-5",0.001,"是"]
[{"$nulls":5},"总磷(mg/L）",{"v":0.2,"d":"0.20"},0.5,"是"]
[{"$nulls":5},"总铅(mg/L）","ND(0.05)",0.1,"是"]
[{"$nulls":5},"总砷(mg/L）","ND(0.01)",0.1,"是"]
["白云区","广州市净水有限公司石井分公司","出水口","2018-10-17","《城镇污水处理厂污染物排放标准》（GB18918-2002）一级A标准+广东省《水污染物排放限值》(DB44/26-2001）第二时段一级标准","pH值（无量纲）",7.12,"6～9","是"]
[{"$nulls":5},"氨氮（mg/L）",0.069,5,"是"]
[{"$nulls":5},"动植物油（mg/L）","ND(0.04)",1,"是"]
[{"$nulls":5},"粪大肠菌群（个/L）","<10",1000,"是"]
[{"$nulls":5},"化学需氧量（mg/L）",5,40,"是"]
[{"$nulls":5},"六价铬（mg/L）","ND(0.004)",0.05,"是"]
[{"$nulls":5},"色度(倍)",4,30,"是"]
[{"$nulls":5},"石油类（mg/L）",0.06,1,"是"]
[{"$nulls":5},"烷基汞（ng/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量（mg/L）",1.5,10,"是"]
[{"$nulls":5},"悬浮物（mg/L）",8,10,"是"]
[{"$nulls":5},"阴离子表面活性剂（mg/L）","ND(0.05)",0.5,"是"]
[{"$nulls":5},"总氮（mg/L）",{"v":4.5,"d":"4.50"},15,"是"]
[{"$nulls":5},"总镉（mg/L）","ND(0.003)",0.01,"是"]
[{"$nulls":5},"总铬（mg/L）","ND(0.01)",0.1,"是"]
[{"$nulls":5},"总汞（mg/L）","5.3×10-5",0.001,"是"]
[{"$nulls":5},"总磷（mg/L）",0.09,0.5,"是"]
[{"$nulls":5},"总铅（mg/L）","ND(0.05)",0.1,"是"]
[{"$nulls":5},"总砷（mg/L）","ND(0.01)",0.1,"是"]
["增城区","广州盈隆污水处理有限公司","污水站处理后","生产负荷不满足监测要求","《水污染物排放限值》(DB44/26-2001）第二时段一级标准","/","/","/","/"]
["增城区","广州新滔水质净化有限公司","出水口","停产","《水污染物排放限值》(DB44/26-2001）第二时段一级标准+表1第一类污染物\n最高允许排放浓度","/","/","/","/"]
["备注：结果中“ND”表示未检出，括号中数值为该项目检出限。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}