{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["污水厂","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"污水厂","index":0,"n_rows":29,"n_cols":9,"rows_kept":29,"merged":[[1,0,1,8],[3,0,27,0],[3,1,27,1],[3,2,27,2],[3,3,27,3],[3,4,27,4]],"flags":["formulas_cached_only"]}
["附件9"]
["广州市2018年国控企业污染源（污水处理厂）监督性监测结果（第4季度）"]
["行政区","企业名称","监测点位","监测日期","执行标准名称","监测项目名称(单位)","污染物浓度","标准限值","是否达标"]
["增城区","广州盈隆污水处理有限公司","污水站处理后","2018-11-06","《水污染物排放限值》(DB44/26-2001）第二时段一级标准","pH值(无量纲)",7.07,"6～9","是"]
[{"$nulls":5},"氨氮（mg/L）",3.63,10,"是"]
[{"$nulls":5},"苯胺类（mg/L）","ND(0.03)",1,"是"]
[{"$nulls":5},"动植物油（mg/L）",0.05,10,"是"]
[{"$nulls":5},"二氧化氯（mg/L）",0.15,"/","/"]
[{"$nulls":5},"粪大肠菌群(个/L)","1.8×103","/","/"]
[{"$nulls":5},"化学需氧量（mg/L）",38,90,"是"]
[{"$nulls":5},"挥发酚（mg/L）",0.01,0.3,"是"]
[{"$nulls":5},"硫化物（mg/L）","ND(0.005)",0.5,"是"]
[{"$nulls":5},"六价铬（mg/L）","ND(0.004)",0.5,"是"]
[{"$nulls":5},"色度(倍)",4,40,"是"]
[{"$nulls":5},"石油类（mg/L）",0.07,5,"是"]
[{"$nulls":5},"烷基汞（mg/L）","ND(1.0×10-5)","不得检出","是"]
[{"$nulls":5},"五日生化需氧量（mg/L）",9.3,20,"是"]
[{"$nulls":5},"悬浮物（mg/L）",18,60,"是"]
[{"$nulls":5},"阴离子表面活性剂（mg/L）",0.07,5,"是"]
[{"$nulls":5},"总氮（mg/L）",5.76,"/","/"]
[{"$nulls":5},"总镉（mg/L）","ND(0.003)",0.1,"是"]
[{"$nulls":5},"总铬（mg/L）","ND(0.01)",1.5,"是"]
[{"$nulls":5},"总汞（mg/L）","ND(9×10-6)",0.05,"是"]
[{"$nulls":5},"总磷（mg/L）",0.08,0.5,"是"]
[{"$nulls":5},"总铅（mg/L）","ND(0.05)",1,"是"]
[{"$nulls":5},"总砷（mg/L）","ND(0.01)",0.5,"是"]
[{"$nulls":5},"总锑（mg/L）","7.4×10-3","/","/"]
[{"$nulls":5},"总铜（mg/L）","ND(0.01)",0.5,"是"]
["备注：结果中“ND”表示未检出，括号中数值为该项目检出限。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}