{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet0"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet0","index":0,"n_rows":22,"n_cols":8,"rows_kept":22,"merged":[[0,0,0,7]],"flags":["formulas_cached_only"]}
["2023年广州市生态环境执法随机抽查情况公示表"]
["序号","污水处理厂\n名称","企业类型","检查时间","检查情况","是否发现问题","检查结果","处理结果"]
["1","广州市净水有限公司沥滘分公司","重点监管对象","2023-12-22","环评制度落实：已检查，未发现异常；“三同时”制度落实：已检查，未发现异常；排污许可证制度落实：已检查，未发现异常；治污设施运行情况：已检查，未发现异常；污染物排放情况：已检查，未发现异常","否","未发现环境问题","/"]
["2","广州市净水有限公司大坦沙分公司","重点监管对象","2023-12-26","荔湾分局对该单位污水处理设施，污水在线监控系统，危废及一般工业固废工作台账及贮存场所、突发环境事件应急预案开展现场检查，未发现环境违法行为。","否","未发现环境违法行为","/"]
["3","广州市净水有限公司大观分公司","重点监管对象","2023-12-25","现场检查时，企业正常生产，执法人员现场检查该企业实验室、在线监控、危险废物贮存等，未发现问题。","否","未发现问题终止检查并向监管对象告知检查结果","/"]
["4","广州市净水有限公司猎德分公司","重点监管对象","2023-12-25","现场检查时，企业正常生产，执法人员现场检查该企业实验室、在线监控、危险废物贮存等，未发现问题。","否","未发现问题终止检查并向监管对象告知检查结果","/"]
["5","广州市净水有限公司石井净水分公司","重点监管对象","2023-12-19","现场检查情况：发现该企业生产过程中有废水，废气产生，废水经污染物治理设施处理后排入外环境，废气经生物除臭，活性炭吸附装置处理后排放，已取得排污许可证。检查时当事人正在生产，污染治理设施正在运行，自动在线监测设施数据无异常。","否","未发现问题终止检查并向监管对象告知检查结果 ","/"]
["6","广州市净水有限公司石井分公司","重点监管对象","2023-12-19","现场检查情况：发现该企业污水尾水已安装在线监控，在线由深圳浩瑞泰科技有限公司负责运营，污水在线正常运行，各项监控污染因子正常。","否","未发现问题终止检查并向监管对象告知检查结果 ","/"]
["7","广州科学城水务投资集团有限公司（西区水质净化厂）","重点监管对象","2023-12-28","现场检查时，该企业正常生产，污染治理设施正常运行，环保手续齐全；检查时废气处理系统故障应急处置、废水处理系统泄漏应急处置演练未开展，已督促该厂及时开展针对性演练。","是","检查时发现：突发环境应急演练有两项演练内容未开展","责令整改"]
["8","广州科学城水务投资集团有限公司（生物岛再生水厂）","重点监管对象","2023-12-28","现场检查时，该企业正常生产，污染治理设施正常运行，环保手续齐全；现场检查未发现该污水厂存在环境违法行为。","否","现场检查未发现环境违法行为。","/"]
["9","广州科学城水务投资集团有限公司（九龙水质净化三厂）","重点监管对象","2023-12-27","现场检查时，该企业正常生产，污染治理设施正常运行，环保手续齐全；现场检查未发现该污水厂存在环境违法行为。","否","未发现环境违法行为","/"]
["10","广州市花都排水有限公司（梯面镇污水处理厂）","重点监管对象","2023-12-25","现场正常运行，水质在线监测正常，出水感官清澈。环保手续资料齐全，落实排污许可制度，近期监测报告达标。","否","情况正常","/"]
["11","广州市花都净水有限公司（梯面镇污水处理厂联丰污水处理站）","重点监管对象","2023-12-25","现场已停止污水处理，仅有污水提升泵功能。","否","情况正常","/"]
["12","广州白云国际机场股份有限公司（机场污水处理站）","重点监管对象","2023-12-25","1.企业已办理环评手续，完成验收，取得排污许可证；\n2.企业水处理设施正常运行；\n3.企业污泥交由越堡水泥有限公司处理。","否","情况正常","/"]
["13","广州市番禺污水治理有限公司（前锋净水厂）","重点监管对象","2023-12-21","检查时该单位正常生产，总排水口正在外排，在线监控数据为：一号渠出水瞬时流量4460.323m3/h,累计流量8120048.000m3，二号渠出水瞬时流量5519.603m3/h，累计流量6624638.000m3；COD20.853mg/L;氨氮0.0559mg/L；总氮12.260mg/L；总磷0.4070mg/L。三号渠出水瞬时流量5375.802m3/h,累计流量6370849.500m3。","否","未发现问题","/"]
["14","广州市番禺污水治理有限公司（钟村净水厂）","重点监管对象","2023-12-20","现场检查时，该单位正常生产，废气、废水治理设施正常运行。在线监控数据显示（出水口）(12-20-10:45)，该单位pH：6.52，挥发酚：0.0002ug/L，总氮：10.88mg/L，总磷：0.1123mg/L，氨氮：1.5381mg/L，化学需氧量：19.13mg/L，瞬时流量值：3741.4497L/s，累计流量值：8755692立方米。现场检查时该单位2台燃天然气锅炉已完成低氮改造工程。","否","未发现问题","/"]
["15","广州南沙华浩水处理有限公司","重点监管对象","2023-12-28","该污水处理站在2010年11月取得环评批复（穗南区环管影［2010］232号），2013年2月取得环保验收批文（穗南开环管验［2013］10号）。该单位主要收集处理的污水为:工业园内企业排放的污水、周边楼盘生活污水、珠江街道部分生活污水。其处理工艺为：进水-粗格栅-提升泵站-细格栅-旋流沉沙池-厌氧池-缺氧池-好氧池-二沉池-提升泵站-纤维过滤池-紫外消毒-排水。该公司已建在线监控系统。\n现场检查，该公司污水处理设施正在运行，能提供污水设备运营台账及设备维护台账，未发现环境违法行为，已要求该公司加强监督管理，确保污水达标排放。","否","未发现环境问题","/"]
["16","广州科涤水处理有限公司（榄核净水厂）","重点监管对象","2023-12-28","该污水处理站在2009年10月通过环评，2012年2月通过自主验收，2021年12月申领排污许可证（91440115MA59BWTH59004Q），有效期至2026年12月24日。该单位主要收集处理的污水为：城市污水。其处理工艺为：进水-细格栅及旋流沉沙池-CAST生化池-高效沉淀池-纤维转盘滤池-接触消毒池-尾水排放。该公司已建在线监控系统。\n现场检查时，该公司污水处理设施正在运行，能提供污水设备运营台账及设备维护台账，发现一般环境违法行为，危废房分区标志信息不全，缺少废空桶的分区信息。已要求企业整改上述违法行为，加强日常监督管理，确保污水达标排放。","是","发现一般环境违法行为","责令整改"]
["17","广州市从化水质净化厂","重点监管对象","2023-12-28","现场检查，该水质净化厂正在生产运行，一期工程规模设计污水处理能力为0.22万吨，二期工程规模设计处理能力为1.38万吨，采用AA/O生化处理工艺，出水水质执行国标一级A级标准。经查阅监测报告，水质达标排放。","否","暂未发现环境问题","/"]
["18","太平污水处理厂","重点监管对象","2023-12-28","现场检查时，太平污水处理厂正在对mbr膜进行清洗，清洗污水进入污水收集池，现场发现收集不够完善，要求立即整改。","是","发现一般环境问题","责令整改"]
["19","广州海滔环保科技有限公司","重点监管对象","2023-12-26","该公司正常生产，污染物治理设施正常运行.现场检查发现该公司污泥暂存间大门未关闭等问题，要求该公司立行立改","是","发现一般环境问题","立行立改"]
["20","广州增城北控水处理有限公司（中心城区净水厂）","重点监管对象","2023-12-29","该公司正常生产，污染物治理设施正常运行。检查发现进水、出水采样管道未粘贴标示，要求该公司立行立改。","是","发现一般环境问题","立行立改"]